Create a 5 LED chaser

A picture containing text, electronics

Description automatically generated

void setup()

{

pinMode(6, OUTPUT);

pinMode(5, OUTPUT);

pinMode(4, OUTPUT);

pinMode(3, OUTPUT);

pinMode(2, OUTPUT);

}

void loop()

{

digitalWrite(6, HIGH);

delay(100);

digitalWrite(6, LOW);

delay(100);

digitalWrite(5, HIGH);

delay(100);

digitalWrite(5, LOW);

delay(100);

digitalWrite(4, HIGH);

delay(100);

digitalWrite(4, LOW);

delay(100);

digitalWrite(3, HIGH);

delay(100);

digitalWrite(3, LOW);

delay(100);

digitalWrite(2, HIGH);

delay(100);

digitalWrite(2, LOW);

delay(100);

digitalWrite(3, HIGH);

delay(100);

digitalWrite(3, LOW);

delay(100);

digitalWrite(4, HIGH);

delay(100);

digitalWrite(4, LOW);

delay(100);

digitalWrite(5, HIGH);

delay(100);

digitalWrite(5, LOW);

delay(100);

digitalWrite(6, HIGH);

delay(100);

digitalWrite(6, LOW);

delay(100);

}